PRODUCTS & SYSTEMS 


PRODUCTS & SYSTEMS          			Page 1 of 8


SECTION 07 42 13
Custom LockAlign™ Metal Wall Panels 

Go to https://www.azahner.com/document-library/ to verify that this is the most current version of the specification.

Use in conjunction with LockAlign™ Panel datasheet https://www.azahner.com/document/LockAlign-datasheet/

Contact Zahner for assistance with specifications and detail coordination: https://www.azahner.com/contact/

Optional items requiring selection by the specifier are in [blue]. Once selections are made and other options and brackets deleted, bold font and colored text should be reverted to match the balance of the document.

GENERAL
SECTION INCLUDES
LockAlign™ custom interlocking [stainless steel] [weathering steel] [carbon steel] [aluminum] metal panels, fabricated to project-specific dimensions.
[Optional – adjustable z-girts that allow space for insulation between the metal panel and outer plane of the wall assembly.]
RELATED SECTIONS
Division 1 – General Requirements
Submittal Procedures
Quality Control
Closeout Submittals
Division 5 – Metal
Cold-Formed Metal Framing (substrate framing) - not included and needs to be installed prior to LockAlign™ Panel system installation.
Division 6 – Wood, Plastics, and Composites
Rough Carpentry (plywood sheathing) - not included and needs to be installed prior to LockAlign™ Panel system installation.
Division 7 – Thermal and Moisture Protection
Waterproofing - not included and needs to be installed prior to LockAlign™ Panel system installation.
Thermal Insulation - not included and needs to be installed prior to LockAlign™ Panel installation.
REFERENCE STANDARDS - Work shall comply with published recommendations of the following unless otherwise stated below:
ZAHNER “Architectural Metals – A Guide to Selection, Specification and Performance”; John Wiley & Sons 1995: ISBN 0-471-04506-3.
ZAHNER “Architectural Metal surfaces”; John Wiley and Sons 2005: ISBN 0-47126335-4.
SMACNA “Architectural Sheet Metal Manual”.
LEED – Leadership in Energy and Environmental Design.
ASTM International

[stainless steel] ASTM A240: Standard Specification for Chromium and Chromium-Nickel Stainless Steel Plate, Sheet, And Strip for Pressure Vessels And For General Applications.
[stainless steel] ASTM A480: Standard Specification for General Requirements for Flat Rolled Stainless and Heat-Resisting Steel Plate, Sheet, and Strip.
[bookmark: _Hlk197350843][weathering steel] ASTM A588: Standard Specification for High-Strength Low-Alloy Structural Steel, up to 50 ksi Minimum Yield Point, With Atmospheric Corrosion Resistance.
[weathering steel] ASTM A606: Standard Specification for Steel, Sheet and Strip, High-Strength, Low-Alloy Hot Rolled and Cold Rolled, With Improved Atmospheric Corrosion Resistance.
[carbon steel] ASTM A1008: Standard Specification for Steel, Sheet and Strip, Cold-Rolled.
[aluminum] ASTM B209: Standard Specification for Aluminum and Aluminum-Alloy Sheet and Plate.
[aluminum] ASTM D2244: Standard Practice for Calculation of Color Tolerances and Color Differences from Instrumentally Measured Color Coordinates.
[aluminum] ASTM D4214: Standard Test Methods for Evaluating the Degree of Chalking of Exterior Paint Films.
AAMA – American Architectural Manufacturers Association (www.aamanet.org).
[aluminum] AAMA 611: Voluntary Specification for Anodized Architectural Aluminum.
[aluminum] AAMA 2605 & 2604: Voluntary Specification, Performance Requirements and Test Procedures for Superior Performing Organic Coatings on Aluminum Extrusions and Panels.
[aluminum] AAMA 609 & 610: Cleaning and Maintenance Guide for Architectural Finished Aluminum. 
SUBMITTALS
Product Data: Submit manufacturer's Product Datasheet and installation instructions for custom LockAlign™ Metal Panels, including material, finish, panel thickness, panel dimensions, reveal dimensions, system depth, and patterning layout. 
Samples:
Finish Selection Sample: If requested, provide up to 5 of each material finishes for Architect’s selection. Minimum Sample sizes: 
[Angel Hair® Stainless Steel] [GB-60™ Stainless Steel] [Fuscara™ Blackened Stainless Steel] [Solanum™ Weathering Steel] [Oscura™ Blackened Steel]: 8” x10” 
70% PVDF fluoropolymer paint chip Aluminum: 2” x 2”
Anodized Aluminum: 1” x 3”
Formed Sample: If requested, provide a formed representative sample, no larger than 24” x 24”. The formed edges shall demonstrate the LockAlign™ Panel design. Sample will be provided in the material specified but may not include finish. 
Shop Drawings: Submit shop drawings detailing installation layouts, panel centerline dimensions, connections, and minimum fastener spacing. Architect to provide all electronic CAD files for the basis of shop drawings.
Patterning Files: Submit panel layout files based on the pattern provided by the Architect. 
Technical Datasheet: Submit technical data, including but not limited to pre-engineered structural calculation, system weight, and design pressure. [Project specific engineering certification can be provided by the manufacturer at additional cost.]
Closeout Submittals: 
Warranty: Warranty documents specified herein.
Operation and Maintenance Instructions: Submit manufacturer's recommended cleaning and care instructions to properly maintain and prolong the service life of the metal panels. 
Sustainable Design Submittals (LEED Reports):
Submit documentation from manufacturer for amount of pre-consumer and post-consumer recycled content for products specified.
Submit documentation providing location of manufacturing.
QUALITY ASSURANCE
Field Measurements: Contractor is responsible for providing final overall dimensions of the work surface area(s) prior to shop drawing submittal. At the Contractor discretion, this may be field verified dimensions. Information must be supplied in a format acceptable to the manufacturer.
Manufacturer Qualifications: Company specializing in manufacturing the quality products specified in this section with at least 15 years of documented experience and sufficient capacity to produce the required units within the Project Schedule.
Installer Qualifications: 
Company specializing in installing the work of this section with at least 5 years of documented experience with comparable size project.
Familiar with the Products and the manufacturer’s installation methods.
Source Limitation:
When possible, ensure all raw material came from the same producing mill, the same master slab, and the same chemical composition. 
All panels in this section shall be produced by the same manufacturer and finished by the same finish applicator to protect against variations. 
DELIVERY, STORAGE, AND HANDLING 
Delivery and Receipt:
Deliver products in factory sealed and labeled packages. 
All crates and packaging should be inspected upon delivery for damage. Contact the manufacturer immediately at the time of receipt if any damage is identified. Photographs of any damaged product, including concealed damages, must be supplied to the manufacturer with any claims. Photos of damaged crates and packaging must also be provided to manufacturer.  Freight damage must be filed with freight company within the freight carrier’s terms.
Storage and Transportation:
Keep packaging units dry while in secure and locked storage and transport.
Keep panels dry prior to installation.
Crated products that are stored under tarps should be frequently opened and ventilated to reduce humidity and condensation accumulation.
Do not lay any protective mats or covers directly on top of panels.
Do not store panels in contact with other materials that might cause staining, denting, or other surface damage.
Crates and packaging: Do not stack crates unless otherwise approved and noted by manufacturer.
[Fuscara™ Blackened Stainless Steel] [Solanum™ Weathering Steel] [Oscura™ Blackened Steel] Do not lay any exposed and finished face against another surface or another panel for any length of time. Water will accumulate between the surfaces and cause an accelerated oxidation on the patina.
Handling and Installation: 
Keep film-protected products dry and out of direct sunlight until installation.
Remove the protective film immediately after installation.
Require all personnel to wear clean white cotton gloves when handling and installing architectural metal panels.
Keep product free of oil, grease, mortar, paint, acid, bitumen, drilling dust, dirty water, and other impurities.
Do not use adhesive tape on products in areas visible after installation.
Do not scribe or mark on products.
Protection:  The Contractor is responsible to use all means necessary to protect the materials of this Section before, during and after installation and to protect the installed work and materials of all other trades.
Site Conditions: Adjoining substrate and structure for attachment to be complete. Installation subject to state of inclement weather.
Replacements: In the event of damage, immediately make all repairs and replacements necessary at the sole cost of the responsible party.
WARRANTY 
Manufacturer’s Warranty: Manufacturer will warrant its products to be in good quality, free from defects, in conformance with the specification, and when installed in accordance with manufacturer’s published installation procedures. Any defaults or defects in material or workmanship resulting solely from the manufacturer shall constitute a warranty claim. Manufacturer’s warranty coverage and failure types includes, but not limited to, the following: 
2-years limited warranty for all structural failures including, but not limited to, permanent deflection beyond design limit.
1-year limited warranty on deterioration of metals, defined as perforation due to corrosion resulting from manufacturer’s defects, and loss of adhesion as a result from manufacturer’s finish application. Damage to or failure of the product caused by the improper handling or cleaning will not be covered. This warranty does not cover natural weathering and fading of the surface that will occur as the surface is exposed to ambient conditions. Nor does it cover minor oxidation or oxidation products that transfer to other surfaces.
Warranty commences upon shipment of material by manufacturer.
During the warranty period, and upon approval of the claim, the manufacturer will repair, or at its option, replace the products that are proven to be defective. The labor and all associated costs (i.e., Scaffolding, lifts, etc.) to remove and reinstall repaired or replacement product is not included. 
Finish Applicator’s Warranty: 
[Angel Hair® Stainless Steel] [GB-60™ Stainless Steel] [Fuscara™ Blackened Stainless Steel] [Solanum™ Weathering Steel] [Oscura™ Blackened Steel] See manufacturer applied finish. See 1.7 A.2 above.
[aluminum] AAMA 2605 2-coat solid color 70% PVDF fluoropolymer coating:
Finish Period: Standard 1-year warranty from Finish Applicator’s Warranty Effective Date [Also available in 5, 10, or 20 years, but requires advanced request and at additional cost].
Warranty Coverage: 
Coating will not chalk in excess of numerical rating eight (8) for colors and six (6) for whites, when measured in accordance with ASTM D4214 procedures.
Coating will not fade or change in color in excess of 5 units (Hunter color difference) if calculated from measurements on any spectrophotometer or colorimeter designed to adequately measure color by reflectance readings in accordance with ASTM D2244 test method 6.3. 
Coating will not crack, check or peel (lose adhesion). This does not include minute fracturing, which may occur during fabrication, installation, or use of the metal.
AAMA 611 Class I anodized aluminum: 
Finish Period: Standard 1-year warranty from Finish Applicator’s Warranty Effective Date [Also available in 5 or 10 years, but requires advanced request and at additional cost]
Warranty Coverage: 
1. No chalking. This only applies to any powdery residue formed by the breakdown of the anodized finish. It does not apply to any foreign residue deposited on the surface of the anodized finish by the surrounding atmosphere (soot, dust, etc.). 
No significantly visible fading or change in color in excess of 5 units (Hunter color difference), measured by the same test method referenced in B the section above.
No visible peeling or cracking. This excludes any crazing microfracture due to brake bends or other forming operations.
PRODUCT
MANUFACTURERS
Basis of Design: A. Zahner Company LockAlign™ Panel System
[bookmark: _Hlk197340399]Product Website: https://www.azahner.com/products/LockAlign
Address: 1400 E. 9th Street, Kansas City, MO 64106 
Phone: +1 (816) 423-8354
Request for substitutions will be considered in accordance with provisions in [Section 01 60 00]
PERFORMANCE CRITERIA
System Capabilities
Factory fabricated prefinished metal panel system.
Product shall utilize LockAlign™ system to enable fast and sealant-free installation of metal panels. Primary joint connection shall use factory-fabricated lance and form tabs for secure engagement with the adjacent panel.
Pre-Engineered Design: LockAlign™ panels to be designed to perform at cladding loading criteria established by engineer of record.
Panels shall be designed for secure attachment to continuous substrate or sub girts without visible fasteners.
Panels to be sequenced and numbered without visible notes on the surface to guide a seamless installation process.
Performance Requirements
Design Pressure: In accordance with ASCE 7 and loads indicated on Structural Drawings.
Design and size components to support assembly dead loads, and to withstand live loads caused by positive and negative wind pressure acting normal to the plane of installation.
Movement: Accommodate movement within system without damage to components, movement between system and perimeter components when subject to seasonal temperature cycling; dynamic loading and release of loads; and deflection of structural support framing.
Tolerances
Panels and Components: Panels shall be fabricated to a tolerance not to exceed 1/8” deviation in any dimension from dimensions shown on the shop drawings.
Bent Radius at panel bend should be no more than 4 times the thickness of the metal panel. 
Panel Flatness: Panels shall be fabricated to a flatness that is not to exceed 0.5” out-of-plane when panels are in their installed condition. 
Installation Tolerances: Adjust layout to ensure that panels after installation maintain the tolerance of 1/8” in 10’ that is not cumulative for level, plumb and line. Offset between panel edges shall be less than 1/16” in plane with the surface.
Panel Joints: Panels shall be installed so that panel joints are +/-1/16” of designed reveal.
PANELS
Panel Type: [LockAlign™ Panel] 
Panel Material, Finish, and Thickness
[Angel Hair® Stainless Steel] [GB-60™ Stainless Steel] [Fuscara™ Blackened Stainless Steel] [304 alloy] [316 alloy] 0.075” (14 ga)
[Solanum™ Weathering Steel] [Oscura™ Blackened Steel] 0.075” (14 ga)
5052-H32 Aluminum 0.125”, AAMA 2605 70% PVDF Fluoropolymer coating. 
[Standard 2-coat solid Fluropon] or [Premium [2-coat Fluropon metallic] [3-coat] [4-coat] [Specialty Fluoropolymer] coating also available (additional charges apply)].
5052-H32 Aluminum 0.125”,  AAMA 611 Architectural Class I Anodizing, color or clear anodizing coating of 0.7 mil minimum thickness.
Standard Color: [Clear, Nickel, Champagne, Golden Bronze, Light Bronze, Medium Bronze, Dark Bronze, Deep Bronze, or Electrolytic Black]
Premium Color: [Dyed coating] (additional charges apply).
Panel Width: (installed visible dimension): maximum 40” 
Panel Length: (installed visible dimension): maximum 112”
Panel Depth: 1.5”
ACCESSORIES
Accessories shall be fabricated from corrosion-resistant metals compatible with LockAlign™ Panel material. 
[Optional – adjustable z-girts]: 
[5052-H32 Aluminum [0.125”] [0.190”] thick L-shape, dimensions based on project requirements.]
[304 alloy] [316 alloy] Stainless Steel 0.075 thick L-shape, dimensions based on project requirements.]
Not included by the panel fabricator:
Fasteners connecting LockAlign™ system components to other building components, including substrate.
Fasteners connecting adjustable depth sub-girts to itself, to the LockAlign™ panels, and to other building components, including substrate.
Flashing or fascia components to be fabricated by installer from flat sheet stock in LockAlign™ panel materials and finishes. See 2.3 Panels above.
EXECUTION
SITE CONDITION VERIFICATION
Verify substructure’s location and condition are suitable for installation of the custom panels in accordance with the manufacturer’s specification.
Confirm substructure surface is plumb, true, capable of supporting the custom panel system without deflection or deformation, and that can receive the required fasteners for the LockAlign™ panel system. Correct any conditions detrimental to the proper and timely completion of the work. Do not proceed with the work until unsatisfactory conditions are corrected to permit proper installation of the work. 
FABRICATION
Fabricate LockAlign™ Panels in compliance with the drawing details which include design, dimensions, geometry, metal thickness and other characteristics. 
Allow sufficient room for expansion in the material to prevent buckling, damage, and deterioration of the Work. 
SITE PREPARATION
Examine substrate and ensure surfaces are clean and clear of all obstacles and debris. 
Ensure there is enough space and clearance in the work area to receive the custom metal panels.
INSTALLATION
[Optional – If adjustable z-girts are used, install prior to panel installation in accordance with manufacturer's instructions. Ensure z-girts are plumb, true, and securely fastened to the substrate at spacing required to support the panel system.]
Comply with panel manufacturer's instructions for assembly, installation, and erection of custom metal panels.
Install LockAlign™ panels square, plumb, straight, and true.
TOLERANCE
Localized substructure tolerance – 1/4” maximum.
[bookmark: _Hlk197347197]Installation Tolerances: Layout panel joint to ensure centerline of panel reveal tolerances do not exceed +/- 1/8” from approved drawings. Adjust layout to ensure that panels after installation maintain the tolerance of 1/8” in 10’ that is not cumulative for level, plumb, and line. Offset between panel edges shall be less than 1/16” in plane with the surface.
CLEANING AND PROTECTION
Remove protective film from exposed surfaces of metal panels promptly upon installation and in accordance with manufacturer’s recommendations and with care to avoid damage to finish.
Clean exposed surfaces of custom metal panel work promptly after completion of installation. Comply with the recommendations of the panel manufacturer.
Maintain installed custom panels in a clean condition throughout construction and ensure that cleaning by other trades in proximity to the custom panels does not impart dust or debris on panels. Avoid spilling, dripping, or splattering cleaning solutions onto custom panels.

End of Section

LockAlign™ Panel Specification | August 28, 2026
		
	


LockAlign™ Panel Specification | August 28, 2026		


image1.png




image2.svg
                    


image3.jpg




