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SECTION 09 78 13
Zahner Moda Metal Panel System 

Go to azahner.com/document-library/ to verify that this is the most current version of the specification.

It is recommended to use this specification in conjunction with the following documents:
1. Moda Datasheet azahner.com/document/moda-order-form/
2. Moda Installation Manual azahner.com/document/moda-installation-manual/
3. Zahner Sheet Material 3-part specification azahner.com/document/surfaces-specification/
4. [bookmark: _Hlk198282099]Moda Panel Planner azahner.com/document/moda-panel-planner/

Contact Zahner for assistance with specifications and detail coordination: azahner.com/product-inquiries/#contact

Optional items requiring selection by the specifier are in [blue]. Once selections are made and other options and brackets deleted, bold font and colored text should be reverted to match the balance of the document.

GENERAL
SECTION INCLUDES
Pre-fabricated, modular, metal interior wall panel system with related mounting hardware and accessories.
RELATED SECTIONS
Division 1 – General Requirements  
Submittal Procedures
Quality Control
Closeout Submittals
Division 5 – Metal Fabrications
Miscellaneous metal flashing is not included in the system. Sheet material stock may be procured from Zahner if needed.
Division 9
Section 09 77 00 – Special Wall Surfacing
Division 26 – Electrical
Section 26 05 19 – Low-Voltage Electrical Power Conductors and Cables.
Section 26 05 33 – Raceways and Boxes for Electrical Systems.
Section 26 27 26 – Wiring Devices.
Section 26 51 00 – Interior Lighting.
Section 26 09 23 – Lighting Control Devices.
Division 26 work includes:
Branch circuit wiring.
Raceways and junction boxes external to panel assemblies.
Drivers, power supplies, and controls not furnished as part of the Moda system.
Line-voltage and low-voltage wiring between building electrical systems and panel connection points.
Final electrical connections.
Lighting controls integration, commissioning, and testing.
REFERENCE STANDARDS - Work shall comply with published recommendations of the following unless otherwise stated below:
ZAHNER “Architectural Metals – A Guide to Selection, Specification and Performance”; John Wiley & Sons 1995: ISBN 0-471-04506-3.
ZAHNER “Architectural Metal surfaces”; John Wiley and Sons 2005: ISBN 0-47126335-4.
SMACNA “Architectural Sheet Metal Manual”.
ASTM B370: Standard Specification for Copper Sheet and Strip for Building Construction.
ASTM B69: Standard Specification for Rolled Zinc.
ASTM A240: Standard Specification for Chromium and Chromium-Nickel Stainless Steel Plate, Sheet, And Strip for Pressure Vessels And For General Applications.A
ASTM A480: Standard Specification for General Requirements for Flat Rolled Stainless and Heat-Resisting Steel Plate, Sheet, and Strip.
[bookmark: _Hlk197350843]ASTM A1008/A1008M: Specification for Steel, Sheet, Cold-Rolled, Carbon, Structural, High-Strength Low-Alloy, High-Strength Low-Alloy with Improved Formability, Solution Hardened, and Bake Hardenable.
ASTM B209: Standard Specification for Aluminum and Aluminum-Alloy Sheet and Plate.
SUBMITTALS
Product Data: Submit manufacturer's Product Datasheet azahner.com/document/moda-product-datasheet/ and Installation Manual azahner.com/document/moda-installation-manual/.  Indicate:
Panel size(s).
Panel material(s)
Reveal cover material(s)
Panel layout. 
Samples:
Finish Selection Sample: If requested, provide each material and finish for Architect’s selection. Sample size: [8” x 10”]
[Optional Mock-up Panel]: If requested, provide an 18” x 36” mock-up panel and any accessories to establish a quality standard for fabrication and installation. Subject to compliance with the requirement and approval, the mock-up panels [may or may not] become part of the completed Work.
Panel Layout: Submit panel installation layout with panel sizes, orientations and hardware and accessories indicated along with nominal dimensions. Architect to provide all electronic CAD files for the basis of layout. azahner.com/document/moda-panel-planner/
Acoustical Certifications: Manufacturer's certifications that products comply with specified requirements, including laboratory reports showing compliance with specified tests and standards. For acoustical performance, each carton of material must carry an approved independent laboratory classification, such as Underwriter’s Laboratory (UL), of NRC, CAC, and AC.
If the material supplied by the subcontractor does not have an independent laboratory classification of acoustical performance on every carton, subcontractor shall be required to send material from every production run appearing on the job to an independent or NVLAP approved laboratory for testing, at the architect's or owner's discretion. All products not conforming to manufacturer's current published values must be removed, disposed of, and replaced with complying product at the expense of the Contractor performing the work.
Technical Datasheet: Submit technical data, including but not limited to pre-engineered structural calculation, system weight, and maximum design pressure. [Project Specific engineering certification can be provided by the manufacturer at additional cost.]
Closeout Submittals: 
Warranty: Warranty documents specified herein.
Operation and Maintenance Instructions: Submit manufacturer's recommended cleaning and care instructions to properly maintain and prolong the service life of the metal panels. 
Sustainable Design Submittals (LEED Reports):
[Angel Hair Stainless Steel] [GB-60 Stainless Steel] [Solanum Steel] [Oscura Blackened Steel] [Spectura Steel] Submit Product Specific (Type III) Environmental Product Declaration (EPD). 
[Angel Hair Stainless Steel] [GB-60 Stainless Steel] [Solanum Steel] Submit IFLI Declare label. 
Submit documentation from manufacturer for amount of pre-consumer and post-consumer recycled content for products specified.
Submit documentation from manufacturer certifying International Living Future Institute membership, Declare label and Red List Free status.
Submit documentation that certifies compliance with the Buy American Act 41 U.S.C 10a – 10d.
Submit documentation of compliance with environmental requirements of a ‘zero-discharge’ facility.
Integrated Lighting Shop Drawings:
Submit lighting coordination drawings indicating:
Light-integrated panel locations.
Driver and power supply locations.
Junction box locations.
Access requirements for maintenance.
Electrical connection points.
Power and control wiring pathways.
Coordination requirements with Division 26 work.
QUALITY ASSURANCE
Fire Performance Characteristics: Identify ceiling components with appropriate markings of applicable testing and inspecting organization.
Surface Burning Characteristics: As follows, assessed per ASTM E 84 and complying with ASTM E 1264 for Class A products.
Flame Spread: 25 or less
Smoke Developed: 50 or less
Field Measurements: Contractor is responsible for providing final overall dimensions of the work surface area(s) prior to shop drawing submittal. At the Contractor discretion, this may be field verified dimensions. Information must be supplied in a format acceptable to the manufacturer.
Manufacturer Qualifications: Company specializing in manufacturing the quality products specified in this section with at least 15 years of documented experience and sufficient capacity to produce the required units within the Project Schedule.
Installer Qualifications: 
Company specializing in installing the work of this section with at least 5 years of documented experience with comparable size project.
Familiar with the Products and the manufacturer’s installation methods.
Source Limitation:
When possible, ensure all raw material came from the same producing mill, the same master slab, and the same chemical composition. 
All panels in this section shall be produced by the same manufacturer to protect against variations. 
DELIVERY, STORAGE, AND HANDLING 
Delivery and Receipt:
Deliver products in factory sealed and labeled packaging. 
All crates and packaging should be inspected upon delivery for damage. Contact the manufacturer immediately at the time of receipt if any damage is identified. Photographs of any damaged product, including concealed damages, must be supplied to the manufacturer with any claims. Photos of damaged crates and packaging must also be provided to manufacturer.  Freight damage must be filed with freight company within the freight carrier’s terms.
Storage and Transportation:
Keep packaging units dry while in secure and locked storage and transport.
Keep panels dry prior to installation.
Crated products that are stored under tarps should be frequently opened and ventilated to reduce humidity and condensation accumulation.
Do not lay any protective mats or covers directly on top of panels.
Do not store panels in contact with other materials that might cause staining, denting, or other surface damage.
Crates and packaging: Do not stack crates unless otherwise approved and noted by manufacturer.
Do not lay any exposed and finished face against another surface or another panel for any length of time. Water will accumulate between the surfaces and cause an accelerated oxidation on the patina. 
Handling and Installation: 
Keep film-protected products dry and out of direct sunlight until installation.
Remove the protective film immediately after installation.
Require all personnel to wear clean white cotton gloves when handling and installing architectural metal panels.
Keep product free of oil, grease, mortar, paint, acid, bitumen, drilling dust, dirty water, and other impurities.
Do not use adhesive tape on products in areas visible after installation.
Do not scribe or mark on products.
Protection:  The Contractor is responsible to use all means necessary to protect the materials of this Section before, during and after installation and to protect the installed work and materials of all other trades.
Site Conditions: Adjoining substrate and structure for attachment to be complete. Installation subject to state of increment weather.
Replacements: In the event of damage, immediately make all repairs and replacements necessary at the sole cost of the responsible party.
WARRANTY 
Manufacturer’s Warranty: Manufacturer will warrant its products to be in good quality, free from defects, in conformance with the specification, and when installed in accordance with manufacturer’s published installation procedures. Any defaults or defects in material or workmanship resulting solely from the manufacturer shall constitute a warranty claim. Manufacturer’s warranty coverage and failure types includes, but not limited to, the following: 
2-years limited warranty for all structural failures including, but not limited to, permanent deflection beyond design limit.
1-year limited warranty on deterioration of metals, defined as perforation due to corrosion resulting from manufacturer’s defects, and loss of adhesion as a result from manufacturer’s finish application. Damage to or failure of the product caused by the improper handling or cleaning will not be covered. This warranty does not cover natural weathering and fading of the surface that will occur as the surface is exposed to ambient conditions. Nor does it cover minor oxidation or oxidation products that transfer to other surfaces.
Warranty commences upon shipment of material by manufacturer.
During the warranty period, and upon approval of the claim, the manufacturer will repair, or at its option, replace the products that are proven to be defective. The labor and all associated costs (i.e., Scaffolding, lifts, etc.) to remove and reinstall repaired or replacement product is not included. 
Finish Applicator’s Warranty: 
See manufacturer applied finish. See 1.06 A 2. above.

PRODUCT
MANUFACTURERS
Basis of Design: A. Zahner Company Moda Panel System
Product Website: https://www.azahner.com/products/modular-wall-panel-system
Address: 1400 E. 9th Street, Kansas City, MO 64106 
Phone: +1 (816) 423-8354
Substitutions. [None Allowed] [Subject to Performance Criteria] [Request for substitutions will be considered in accordance with provisions in Section 01 60 00]
PERFORMANCE CRITERIA
System Capabilities
Factory-fabricated, prefinished modular metal panel system, site-installed.
Panel system to accommodate vertical (portrait), or horizontal (landscape) panel orientations, or a combination of the two.
Panels to incorporate removable and re-orientable back panels to enable on-site adjustment of panel orientation.
Panel system to enable future re-positioning of panels without the requirement to remove or reinstall hardware.
Panel system should allow for secure attachment to continuous substrate without visible fasteners.
Panel system must allow for vertical reveals between panels, up to 3” wide, without visible hardware or fasteners, or compromising visual or structural performance.
Panel layout and orientation shall follow design requirements to meet project aesthetic.
Hardware and accessories shall allow for secure, repeatable installation and clean edge conditions.
Panels to incorporate a security mechanism to prevent unauthorized removal of panels, but that allows for panel removal in cases of maintenance, repair or replacement.
[Ecology Collection: Panel patterns to enable field modification to allow for on-site customization of louver orientation.]
[Aeris Collection: Panel pattern shall be designed to enable a Noise Reduction Coefficient (NRC): 0.65.]

Performance Requirements
Design and size components to support assembly dead loads.
Movement: Accommodate movement within system without damage to components, movement between system and perimeter components when subject to seasonal temperature cycling; dynamic loading and release of loads; and deflection of structural support framing.
Tolerances
Fabrication: Panels shall be fabricated to a tolerance not to exceed 1/8” deviation in any dimension from dimensions shown on the shop drawings.
Radius at panel bend should be no more than 4 times the thickness of the metal panel. 
Panel Flatness: Panels shall be fabricated to a flatness that is not to exceed L/180 for horizontal panels and L/100 for vertical panels.
SYSTEM SCOPE AND ELECTRICAL COORDINATION
Where indicated on Drawings, the architectural wall panel assembly, including integrated lighting elements, shall be furnished as a complete coordinated architectural system by a single manufacturer.
The system shall include panel-integrated lighting components, mounting provisions, internal wire management pathways, access provisions, and related accessories required for a complete installation.
Division 26 work shall be limited to branch circuit wiring, controls, power supplies not furnished as part of the panel assembly, external raceways and junction boxes, and final electrical connections unless otherwise indicated.
Coordinate all electrical connection points, driver locations, access requirements, and maintenance clearances with Division 26 prior to fabrication.
PANELS
Panel Face Material and Finish: 
[Angel Hair Stainless Steel] [Fuscara Blackened Stainless Steel] [Solanum Steel] [Oscura Blackened Steel] [Spectura Steel] [Star Blue Copper] [Dirty Penny Copper] [Baroque Zinc] [Hunter Zinc] [Roano Zinc] by A. Zahner Co., which is detailed and referenced in SECTION 05 70 00 Zahner Surfaces Pre-Finished Metal Sheets (3-Part specifications are available for a full selection of Zahner Surfaces: https://www.azahner.com/document/surfaces-specification/)
(As an alternative, specifier may insert “PART 2 PRODUCTS” section of the Zahner Surfaces Pre-Finished Metal Sheets specification of choice, as opposed to carrying the complete material specification document in the Division 5 project specifications.)
Panel Face Patterns:
None
Ecology Collection [Folia A] [Folia B] [Folia C] [Plashet A] [Plashet B] [Plashet C] [Rivulet A] [Rivulet B] [Rivulet C]
Aeris [Angel Hair Stainless Steel] [Fuscara Blackened Stainless Steel] [Solanum Steel] [Oscura Blackened Steel] [Spectura Steel]
Panel Sizes: 
[18” x 36”] 
[18” x 54”] 
[18” x 90”] 
[18” x 108”]
INTEGRATED LIGHTING COMPONENTS
Where indicated on Drawings, furnish factory-integrated LED lighting assemblies designed for incorporation within the Moda wall panel system.
Lighting assemblies shall be UL Listed or recognized components suitable for architectural integration and interior installation.
Provide factory-installed mounting provisions, brackets, wiring pathways, and access provisions necessary for installation and maintenance.
Provide concealed raceways within panel assemblies where required for internal wire management.
Where drivers are incorporated into the wall panel assembly, provide removable access panels for service.
Provide clearly identified electrical connection points for field connection by Division 26 trades.
Coordinate fixture dimensions, operating temperatures, ventilation requirements, and maintenance clearances with architectural panel design.
Lighting performance characteristics, lumen output, color temperature, dimming protocol, emergency operation requirements, and controls shall be as indicated on Drawings and specified in Division 26.
ELECTRICAL SCOPE RESPONSIBILITY
Panel manufacturer shall furnish fully integrated and complete lighting panel assemblies.
Division 26 shall provide branch circuiting, power supplies not factory furnished, controls, low-voltage control cabling, external junction boxes, and final electrical connections.
ACCESSORIES
Hardware and accessories shall be fabricated from metals compatible with panels to prevent galvanic corrosion or other issues associated with contact between dissimilar metals.  
HARDWARE (delete unnecessary items)
C-Bracket
End Bracket, Left
End Bracket, Right
Corner Bracket, Left
Corner Bracket, Right
End Trim (Product ID: SWJS)
REVEAL COVERS (delete unnecessary items) 
[Angel Hair Stainless Steel] [Fuscara Stainless Steel [304]] [Solanum Steel] [Oscura Blackened Steel] [Spectura Steel] [Star Blue Copper] [Dirty Penny Copper] [Baroque Zinc] [Hunter Zinc] [Roano Zinc] by A. Zahner Co., which is detailed and referenced in SECTION 05 70 00 Zahner Surfaces Pre-Finished Metal Sheets (3-Part specifications are available for a full selection of Zahner Surfaces: https://www.azahner.com/document/surfaces-specification/)
(As an alternative, specifier may insert “PART 2 PRODUCTS” section of the Zahner Surfaces Pre-Finished Metal Sheets specification of choice, as opposed to carrying the complete material specification document in the Division 5 project specifications.)

EXECUTION
SITE CONDITION VERIFICATION
Verify substructure’s location and condition are suitable for installation of the system in accordance with the manufacturer’s specification.
Complete visual inspection of substructure surface to ensure a smooth and continuous surface that can withstand the required loads without deflection or deformation and that is capable of receiving the required fasteners for the panel system. Correct any conditions detrimental to the proper and timely completion of the work. Do not proceed with the work until unsatisfactory conditions are corrected to permit proper installation of the work. 
FABRICATION
Fabricate panels in compliance with the drawing details which include design, dimensions, geometry, metal thickness and other characteristics. 
Allow sufficient room for expansion in the material to prevent buckling, damage, and deterioration of the Work. 
SITE PREPARATION
Examine substrate and ensure surfaces are clean and clear of all obstacles and debris. 
Ensure substrate meets tolerances for line, level, plumb and plane.
COORDINATION
Coordinate panel fabrication with electrical rough-in locations shown on approved shop drawings.
Coordinate electrical connection locations prior to fabrication.
Coordinate placement of drivers, transformers, power supplies, controls, and junction boxes to ensure accessibility after completion of work.
Provide factory-prepared openings, concealed raceways, mounting provisions, and removable access panels required for installation and maintenance of lighting components.
Coordinate sequencing of work with Division 26 to ensure wiring and raceways are installed before panel installation where access will be restricted.
Verify electrical rough-in locations before shipment of fabricated panels.
INSTALLATION
Install lighting-integrated panels in accordance with approved shop drawings and manufacturer's instructions.
Do not conceal junction boxes, drivers, transformers, or electrical components requiring service access.
Cooperate with Division 26 trades during installation to allow wiring and final electrical connections.
Protect lighting components from construction dust, impact, moisture, and contamination during installation.
Replace damaged lighting components at no additional cost to Owner.
Comply with panel manufacturer's instructions for installation of metal panels.
Install hardware system to substrate or back up substructure.
Install hardware square, plumb, straight, and true.
TOLERANCE
[bookmark: _Hlk197347197]Installation Tolerances: Install hardware and panels in accordance with manufacturer’s published installation manual.
Panel Reveals: Panels and hardware to allow for panel joints that are [1/4” (minimum) to 3” (maximum)] +/- 1/8”.
CLEANING AND PROTECTION
Remove protective film from exposed surfaces of metal panels promptly upon installation and in accordance with manufacturer’s recommendations and with care to avoid damage to finish.
Clean exposed surfaces of custom metal panel work promptly after completion of installation. Comply with the recommendations of the panel manufacturer.
Maintain installed custom panels in a clean condition throughout construction and ensure that cleaning by other trades in proximity to the custom panels does not impart dust or debris on panels. Avoid spilling, dripping, or splattering cleaning solutions onto custom panels.


End of Section
 
A. Section 09 77 00 Decorative Metal Wall Panels:
1. Furnished integrated lighting assemblies.
2. Architectural panel supports and mounting provisions.
3. Concealed raceways and access provisions within panel assemblies.
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